## Ladder Inspection Checklist

Date:

Ladder Description:

| **Item To Be Checked** | **Condition O.K.** | **Needs Repair** |
| --- | --- | --- |
| **GENERAL** |  |  |
| Loose steps or rungs (consider loose if they can be moved by hand) |  |  |
| Loose nails, screws, bolts, or other metal parts |  |  |
| Cracked, split or broken uprights, braces, steps or rungs |  |  |
| Slivers on uprights, rungs or steps |  |  |
| Damaged or worn nonslip bases |  |  |
| **STEPLADDERS** |  |  |
| Wobbly (from side strain) |  |  |
| Loose or bent hinge spreaders |  |  |
| Broken Stop on hinge spreaders |  |  |
| Loose hinges |  |  |
| **EXTENSION LADDERS** |  |  |
| Loose, broken, or missing extension locks |  |  |
| Defective locks that do not seat properly when the ladder is extended |  |  |
| Deterioration of rope |  |  |
| **TROLLEY LADDERS** |  |  |
| Worn or missing tires |  |  |
| Wheels that bind |  |  |
| Floor wheel brackets broken, loose or missing |  |  |
| Floor wheels and brackets missing |  |  |
| Ladders binding in guides |  |  |
| Ladder and rail stops broken, loose and missing |  |  |
| Rail supports broken or section of rail missing |  |  |
| Trolley wheels out of adjustment |  |  |
| **TRESTLE LADDERS** |  |  |
| Loose hinges |  |  |
| Wobbly |  |  |
| Loose or bent hinge spreaders |  |  |
| Stop on hinge spreader broken |  |  |
| Center section guide for extension out of alignment |  |  |
| Defective locks for extension |  |  |